
6.                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                  The cleaning and the maintenance
1) The power should be turned off before cleaning and maintaining, preventing accident.
2) After using, the surface of the pop-up toaster can be wiped with a soft damp cloth without corrosive cleaner, while only dry cloth can be applied to control switch.
3) It is prevented from flushing the machine with water against damage.
7. Enclosures

Introduction of the product
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MODEL: ET-T4
         ET-T6
1. Charateristics
The toaster is compact with well designed, providing fast thermal collection and time setting. The machine is surrounded with stainless steel. The toast made by it taste soft and palatable. It can be used either in hotel restaurant or at home. 
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Structure (as shown in the figure)










Mod:ET-T6           Mod:ET-T4
1 The toast slot
2 The slice control switch
3 The power indicating light

4 The time dial
5 The toaster body

6 The toast tray
7 The bread lifter
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3. How to use the toaster
Plug in the toaster, insert bread slices into the slots①, set the dial ④, then the power indicating lamp③ lights, activating the toaster. When hear the ring of 〝ding〞, the toasting cycle is complete. Press the bread lifter⑦, the toast pops up out of the slots. Press the slice control switch② to choose 2 or 4 or 6 bread slices to be toasted at one time for Mod ET-T6 (choose 2 or 4 bread slices for Mod ET-T4).
4. Parameters
	Type
	ET-T4
	ET-T6

	Name
	4-Slice Toaster
	6-Slice Toaster

	Rated load(V)
	220-230V
	220-230V

	Rated power
	1.8(1.1/1.8)KW
	1.8(1.1/2.5)KW

	Time of work
	0-5 minutes
	0-5 minutes

	Slots number
	Four pieces
	Six pieces

	Dimension
	330×285×250mm
	465×285×250mm


5. Circuit diagram
[image: image2.jpg]3.The introduction for using

Inserting on the power. putting the bread into the access D of bc treated bread,
dial the temperature control @ with timing funciion to setting the time of baking
(the indicator light & of power is on here). Then the Toaster over begins to heat
up what'sin it accordingto the time limitset. When hear the ring of "ding", the
Toaster oven would have finished the heating up time of the bread. As long as
pressing the o:1-off for the bread's taking out (), the bread slices will stretch up.
Then press the alternative on-off @ in work, you can adjustthe over's conditions
of working, such as the number of the bread in each baking.

4.The parameters of the facilities

Type ETS-4 ETS-6

Name The Toaster oven of four! The Toaster oven of six
picces pieces

Rated load(V) | 220-230V 220-230V

Rated power 1.8(1.1/1.87 KW 2.5(1.1/1.8/2.5) KW

Time of work 0-5 minutes + 0-5 minutes

Choice in work | Four precces Six preces

Dimension 300x225x2 {5 mm 430x225x215rm

5.Principles of the facilities
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K1 - The time dial            K2 - The slice control switch
HL1 - The power indicating light   R1~R5 - The electric thermal plate  
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